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[bookmark: _Hlk158809742]North America EMV Release Notes
3.1.2xx Series Contact Only


3.1.219.360 – 05/28/2026                                                                 “x” indicates product(s) affected

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: Contactless - Add Capability to Retrieve Tag 9F19 (Token Requestor) from CTLS Reader
	X
	X
	X



3.1.219.340 – 05/18/2026

	[bookmark: _Hlk230944524]Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: Merge from IDPOS - P2PE third party root CA remote upgrade feature (for Open arch Walmart)
	X
	
	

	EMV 3.1 Anthem: SPM reboot function is not working via Diagnostic menu or DX Monitor remote reboot (AnthemPOS only)
	X
	
	

	EMV 3.1 Anthem: Terminal reporting two TransactionResult Events on Early card removal
	X
	X
	X

	EMV 3.1 Anthem: Contactless - Not Functioning - Royal Farms - AX12 - NCR (Display Prompt Should Properly Close Keypad)
	X
	X
	X




3.1.226.1200 – 05/18/20260

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	Back out this change which inadvertently sent a MagStripe “No Card” event when opening chip card reader…

Anthem EMV 3.1: EMV 2.8 v. EMV 3.1 Difference: EMV 2.8 Returns Card Events When Card Reader Opened and Card Already Inserted (EMV 3.1 Does Not)
	X
	X
	X

	EMV 3.1 Jade\SCD:  SCD Startup Unhandled Domain Exception
	
	
	X

	EMV 3.1:  Merge from IDPOS - IDPOS 10 WRSA Walmart MC Fleet Card Failure Due to EMV Tag 56 handling
	X
	X
	X

	Dev - EMV 3.1 GetPOSManufacturer - Return Success="false" if attributes not present
	X
	X
	X

	EMV 3.1 Anthem: Contactless - Not Functioning - Royal Farms - AX12 - NCR (Display Prompt Should Properly Close Keypad)
	X
	X
	X

	EMV 3.1 Anthem: SPM reboot function is not working via Diagnostic menu or DX Monitor remote reboot (ANTPOS only)
	X
	
	

	Dev: EMV 3.1: Merge from IDPOS WRSA- P2PE third party root CA remote upgrade feature (for Open arch Walmart)
	X
	X
	X

	EMV 3.1 Anthem: ANTPOS- Terminal hangs on "One moment please" when submitting an Offline PIN < 4 digits
	X
	X
	X

	Dev -  EMV 3.1: Add "Inundate" Checkbox and Functionality to iXPayTestServer\Client
	X
	X
	X

	EMV 3.1 Open Arch : Some contactless taps are not working due to track error - Null Reference Exception in WayneTap.GetMaskedTrack2Tlv
	X
	X
	X



3.1.226.1040 – 04/16/2026

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: Updated SPM2.5 and SPM2.5V2 OS
OS change: Re-enabled the standard DST feature to restore normal RTC behavior.

Note: this OS should have no effect on units in North America; however, we want the same OS as in EU to be consistent and for unison in production shipments

SPM2.5:
· SPM2.5 Secure PROD: SPM2.5_20260410_Secure_PRO_08252800_26041001
· SPM2.5 Secure DEV: SPM2.5_20260410_Secure_DEV_08254800_26041003
· SPM2.5 Non Secure DEV: SPM2.5_20260410_NonSecure_DEV_08251800_26041002

SPM2.5R:
· SPM2.5R Secure PROD: SPM2.5R_20260415_Secure_PRO_08262900_26041501
· SPM2.5R Secure DEV: SPM2.5R_20260415_Secure_DEV_08264900_26041503
· SPM2.5R Non Secure DEV: SPM2.5R_20260415_NonSecure_DEV_08261900_26041502

	X
	X
	

	EMV 3.1: Anthem, Jade/SCD, T7: Test and Update P2PE config receipt data
	X
	X
	X

	EMV 3.1 Jade SCD: Full software remote upgrade is failing
	
	X
	X



3.1.219.330 – 05/08/2026

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: Merge from IDPOS - P2PE third party root CA remote upgrade feature (for Open arch Walmart)
	X
	
	

	EMV 3.1 Anthem: SPM reboot function is not working via Diagnostic menu or DX Monitor remote reboot (AnthemPOS only)
	X
	
	

	EMV 3.1 Anthem: Terminal reporting two TransactionResult Events on Early card removal
	X
	X
	X

	EMV 3.1 Anthem: Contactless - Not Functioning - Royal Farms - AX12 - NCR (Display Prompt Should Properly Close Keypad)
	X
	X
	X



3.1.219.290 – 04/10/2026

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 Jade SCD: Full software remote upgrade is failing
	
	X
	X



3.1.219.270 – 03/31/2026

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 P2PE: WCrypto, multiple OverrideTrackData Events occur after download file commands
	X
	X
	X




3.1.219.250 – 03/25/2026

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 P2PE: WCrypto, system not sending and OverrideTrackData Event on a successful AdvanceKeyCommand
	X
	X
	X



3.1.219.200 – 03/18/2026

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	Dev - EMV 3.1: SPM2.5 FW - Updated 250901 PROD FW as XAC missed files in initial package
	X
	X
	

	EMV 3.1 Anthem: Murphy AX12 sites are reporting multiple receipts
	X
	X
	X



3.1.219.190 – 03/02/2026

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 P2PE: "Missing Prompt" response after SetPromptDetailsCommand issued
	X
	X
	X

	EMV 3.1 P2PE: Prompts not being displayed when sent via protocol to terminal.
	X
	X
	X

	EMV 3.1: Interac Contact Record02 Test Case Fails Due to Requesting 2nd Gen AC
	X
	X
	X

	EMV 3.1 Anthem: Random SPM disconnects happening at Murphy sites
NOTE:  this ticket adds logging to aid in investigation
	X
	
	

	EMV 3.1 Anthem, T7, Jadescd: GetSupportedBarCodeSymbologiesCommand response differs from 2.8
	X
	X
	X

	Exchange Anthem App and EMV3.1 App capabilities over Remote Messages
	X
	
	



3.1.219.130 – 02/09/2026

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV3.1: IXPayTestServer 3.1.219.XX Not starting on any .219 versions
	X
	X
	X

	EMV 3.1 Anthem: GHS Lab Does Not Properly Return to Idle After 2AM Reboot
	X
	X
	

	EMV 3.1: Interac Contact Test Case Function02 Fails (works on EMV 2.8) - For Bulloch and Infonet
	X
	X
	X

	Dev - EMV 3.1: SPM2.5 FW - Updated 250901 PROD FW as XAC missed files in initial package
	X
	X
	



3.1.219.100 – 01/30/2026

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	Dev - EMV 3.1: P96 - New FW of P96 Card Reader to Correct Mag-Stripe
· P96 FW - Dev -  P96W_Release_83601000_26012601
· P96 FW - Prod - P96W_Release_83601000_26012651

NOTE:  the new P96 260108 FW and later is only compatible with new A20 Rev of the P96 Hardware.  Older FW will NOT work with newer HW (and vice-versa). 

This places P96 in correct build folders
	X
	
	

	EMV 3.1 Anthem: Buc-ee's Production Lab Showing COIPA (3.1.217.2290) - Handle EnableKeypadFunctionKeyCommand Exception Gracefully and Return proper Message
	X
	X
	X



3.1.219.80 – 01/19/2026

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 (Anthem) Image Language Assignment Issue
	X
	
	

	EMV 3.1: TCPMP iOTV Crashes When Processing Large Playlists from GSTV
· Redesign of TCPMP playlist handling to add support for large playlists
	
	X
	X



3.1.219.30 – 12/05/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	Dev - EMV 3.1: P96 - New HW Rev of P96 Card Reader for Bug Fixes (New P96 FW, New SPM2.5OS and new SPM2.5ROS to support new HW)

NOTE:  the new P96 FW is only compatible with new A20 Rev of the P96 Hardware.  Older FW will NOT work with newer HW (and vice-versa). 

· P96 FW - Dev - P96W_Release_83601000_26010801
· P96 FW - Prod - P96W_Release_83601000_26010851
· SPM2.5 OS - Secure Dev - SPM2.5_20251216_Secure_DEV_08254800_25121603
· SPM2.5 OS - Non Secure Dev - SPM2.5_20251216_NonSecure_DEV_08251800_25121602 
· SPM2.5 OS - Secure Prod - SPM2.5_20251216_Secure_PRO_08252800_25121601
· SPM2.5R OS - Secure Dev - SPM2.5R_20251217_Secure_DEV_08264900_25121703 
· SPM2.5R OS - Non Secure Dev - SPM2.5R_20251217_NonSecure_DEV_08261900_25121702
· SPM2.5R OS - Secure Prod - SPM2.5R_20251217_Secure_PRO_08262900_25121701
	X
	
	

	Dev - EMV 3.1 Add P96 Statistics for SPM2.5 and SPM2.5R - Send to SVMX Anthem for DXM
	X
	
	

	EMV 3.1: When the \Flash\PreSystemLog folder is missing , getting the logs from DX monitor takes 2 hours
	X
	X
	X

	EMV 3.1: Send Battery voltage to Anthem over Remote Channel as DiagnosticsDataMetric instead of DiagnosticsDataError
	X
	
	

	Anthem EMV 3.1.217: No PIN Entry Timeout
	X
	X
	X



3.1.219.30 – 12/05/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV Anthem 3.1.217: Softkey Event Sent Before Process Completed (Blocking Shell)
	X
	X
	X

	Dev - EMV 3.1: Proper Logging of EMV Kernel Information for DXMonitor
	X
	X
	X

	Dev - EMV 3.1 Anthem Remote Update: SPM2 Pinpad FW update; SPM2 OS update
	X
	
	

	Dev - EMV3.1:  Log warning for  unexpected encoding type
	X
	X
	X



3.1.219.20 – 12/01/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: SPM2.5R OS Version 251114 - Fixes Data Abort with CTLS Reader
SPM25.R (V2) OS: 251114
	X
	X
	



3.1.218.370 – 12/03/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV Anthem 3.1.217: Softkey Event Sent Before Process Completed (Blocking Shell)
	X
	X
	X



3.1.218.300 – 11/24/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: SPM2.5R OS Version 251114 - Fixes Data Abort with CTLS Reader
SPM25.R (V2) OS: 251114
	X
	X
	



3.1.218.290 – 11/12/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 unable to perform transaction on Verifone (master branch fix)
	X
	X
	X

	Test Server -ADV -dialog box cannot save to modify the data, when hit on the save button
	X
	X
	X

	Dev - EMV 3.1:  P96 - Incorporate Latest PCI6 P96 Card Reader FW into Build - Prevents False Breaches
P96 FW: 251030
	X
	
	



3.1.218.220 – 10/24/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: Card Reader - Not Reading Chip Cards - Phillips 66 - - (EMV Does Not allow Zip Code Secure Prompt During EMV Transaction and GVR Aborts Transaction)
	X
	X
	X



3.1.218.200 – 10/15/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1.218.140: SPM2.5R (V2) not opening card reader when reset (similar to 2am reboot)
· New SPM2.5R (V2) OS - 250930
	X
	
	

	IXEMV: 3.1.218.140 -SPM 2.5R (V2) - Contactless Reader (C150SE) offline when  Reset command (test server) or System Reboot
· New SPM2.5R (V2) OS - 250930
	X
	
	

	EMV 3.1.218 Anthem: AutoUpdate FW MSI Mishandled
· AutoUpdateEU_Anthem New Autoupdate 1.0.2.79
	X
	
	



3.1.218.170 – 9/29/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1.217 (Anthem): P95 Failure After 2am Reboot
	X
	X
	



3.1.218.140 – 9/18/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: P96 - Visa Offline PIN Entry Causes Enter & Clear Key become unresponsive then P96 Card Reader Offline Issue
	X
	
	

	EMV 3.1.217 (Anthem): P95 Failure After 2am Reboot
	X
	X
	

	Dev - EMV 3.1 Add P96 Statistics for SPM2.5 and SPM2.5R - Logging and DXMonitor

P96 FW - dev and prod
· Dev P96W_Release_83601000_25090201
· Prod P96W_Release_83601000_25090251
SPM2.5 OS - with new API call - all three versions
· Dev Non Secure - SPM2.5_20250904_NonSecure_DEV_08251800_25090402
· Dev Secure - SPM2.5_20250904_Secure_DEV_08254800_25090403
· Prod - SPM2.5_20250904_Secure_PRO_08252800_25090401
SPM2.5R OS - with new API call - all three versions
· Dev Non Secure - SPM2.5R_20250904_NonSecure_DEV_08261900_25090402
· Dev Secure - SPM2.5R_20250904_Secure_DEV_08264900_25090403
· Prod - SPM2.5R_20250904_Secure_PRO_08262900_25090401
	X
	
	

	Dev - EMV 3.1: P96 on SPM2.5R- Incorporate New PCI6 P96 Card Reader into Build for SPM2.5R - SPM2.5R OS\FW
	X
	
	

	EMV 3.1 Anthem - AX12 Pilot - Crowfoot Shell - NCR - Payment Issues
	X
	
	

	Dev - EMV 3.1 (Anthem): Battery Voltage to DXMonitor
	X
	X
	X

	DEV - EMV 3.1 Add New Terminal Protocol Message - Get\SetPOSManufacturer
	X
	X
	X



3.1.218.20 – 8/26/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	Dev - EMV 3.1:  Add new SPM2.5FW and SPM2.5RFW to Back Out CRL PCI Support (Not Yet Supported by VirtuCrypt)
· SPM2.5 DEV FW - SPM2.5R_DEV_Jade_Release_21601000_25090202
· SPM2.5R PROD FW - SPM2.5_Jade_Release_21601000_25090101
· SPM2.5R Release Notes - 
· SPM2.5R_DEV_Jade_Release_21601000_25090204
· SPM2.5R Prod FW - SPM2.5R_Jade_Release_21601000_25090203
	X
	X
	



3.1.218.20 – 8/26/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	Dev - EMV 3.1: P96 - Incorporate Latest PCI6 P96 Card Reader FW into Build and new SPM2.5 OS and FW
· P96 FW - Dev - 83601000_25081801
· P96 FW - Prod - 83601000_25081851
· SPM2.5 FW - Dev - 21601000_25073002
· SPM2.5 FW - Prod - 21601000_25073001
· SPM2.5 OS - Secure Dev - 08254800_25081903
· SPM2.5 OS - Non Secure Dev - 08251800_25081902
· SPM2.5 OS - Secure Prod - 08252800_25081901
	X
	X
	

	Dev - EMV 3.1: P96 on SPM2.5R- Incorporate New PCI6 P96 Card Reader into Build for SPM2.5R - SPM2.5R OS\FW
· SPM2.5R DEV FW - SPM2.5R_DEV_Jade_Release_23601000_25080602
· SPM2.5R PROD FW - SPM2.5R_Jade_Release_23601000_25080601
· SPM2.5R Non Secure Dev OS: SPM2.5R_20250822_NonSecure_DEV_08261900_25082202
· SPM2.5R Secure Dev OS - SPM2.5R_20250822_Secure_DEV_08264900_25082203
· SPM2.5R Secure Prod OS - SPM2.5R_20250822_Secure_PRO_08262900_25082201
	X
	X
	

	Anthem :IXEMV -3.1.217.1290 SPM2 Status shows offline or Device is Not connected when updated the Msi Stick
	X
	
	

	[Anthem] EMV 3.1.212.1130 field release version. Keypad fails to enable on DisplaySecurePromptCommand
	X
	
	

	Dev EMV 3.1: Support hostname during SPM pairing process, once paired use hostname to resolve to an IP and then connect to Anthem-Remote Message Server
	X
	
	

	Dev - EMV 3.1: P96 - ServiceUtility Upgrade and AutoUpdater of FW for PCI6 P96 Card Reader
	X
	X
	



3.1.217.2300 – 10/27/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: Card Reader - Not Reading Chip Cards - Phillips 66 - - (EMV Does Not allow Zip Code Secure Prompt During EMV Transaction and GVR Aborts Transaction)
	X
	X
	X



3.1.217.2290 – 9/27/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1.217 (Anthem): P95 Failure After 2am Reboot
	X
	X
	



3.1.217.2280 – 9/17/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1.217 (Anthem): P95 Failure After 2am Reboot
	X
	X
	



3.1.217.2260 – 9/12/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	[Anthem] EMV 3.1.212.1130 field release version. Keypad fails to enable on DisplaySecurePromptCommand
	X
	
	



3.1.217.2250 – 8/22/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 Anthem - AX12 Pilot - Crowfoot Shell - NCR - Payment Issues
NOTE:  this is a work-around for an NCR issue
	X
	X
	X



3.1.217.2240 – 8/12/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	Dev - EMV 3.1 (Anthem): Battery Voltage to DXMonitor
This feature has been removed and will be added in a future release
	X
	X
	X



3.1.217.2190 – 7/14/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1| Shell Lab | Driver ID Issue| Pilot Blocker
	X
	X
	X

	Dev - EMV 3.1 (Anthem): Battery Voltage to DXMonitor
	X
	X
	X




3.1.217.2130 – 6/27/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1.215: P95 Failure after 2am Reboot
	X
	X
	

	Dev - EMV 3.1: Enforce WCrypto Initial Configuration file signing
	X
	X
	X



3.1.217.2020 – 6/27/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	Dev - EMV 3.1: Remove Trailing Spaces on Print Commands from POS in Terminal Protocol Messages
	X
	X
	X



3.1.217.1970 – 6/18/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	Dev - EMV 3.1: Remove Trailing Spaces on Print Commands from POS in Terminal Protocol Messages
	X
	X
	X

	Dev - EMV 3.1: P96 - Incorporate New PCI6 P96 Card Reader into Build
· P96 CAB Files
	X
	X
	



3.1.217.1970 – 6/12/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	Anthem :SPM2, SPM2.5 OS not Updating in usb stick install (MSI file)
Implement new feature to support updating SPM2\2.5 OS via MSI
	X
	
	

	Dev - EMV 3.1: Anthem: Delay persisting terminal params during transaction processing
	X
	
	

	Dev - EMV 3.1: P96 - Incorporate New PCI6 P96 Card Reader into Build
· P96 Firmware – initial firmware for new device 250527
· SPM2.5 OS - Implement P96 feature and API add '4' = P96 NoPCI FW version - 250523 (to support P96)
	X
	X
	



3.1.217.1930 – 5/14/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 Anthem: No possibility to download logs from SPM.
Dev - EMV 3.1: Anthem: Delay or reject logs pull requests during transaction times]
	X
	
	

	Port changes from IDPOS to fix issues with SPM2.5e upgrades
	
	
	X



3.1.217.1900 – 5/7/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	Dev - EMV 3.1: POS and DXM Socket Connections - use IP Address or hostname
	X
	X
	X

	EMV 3.1.215: CustomerCancel Behavior Inconsistent
	X
	X
	X

	EMV 3.1 Anthem: Screen stuck on one moment on pre-selection. This issue comes from Bulloch PKI0702A-73
	X
	X
	X



3.1.216.1840 – 5/7/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: Invalid SPM Application version in 3.1.216.1830. Displaying as Platform version 2.0.1.101.1447
	X
	X
	X



3.1.216.1830 – 4/24/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 Anthem: Shell Canada NCR Not able to Cancel transaction when Select Car Wash prompt is displayed
	X
	X
	X

	Dev - EMV 3.1: Anthem: Delay or reject logs pull requests during transaction times
	X
	
	

	EMV 3.1 Anthem OpenArch:  EMV Single Application Confirmation Card Does Not Complete
	X
	
	

	Dev - EMV 3.1 Anthem: Populate PackageVersion attribute in GetPackageVersionResponse
	X
	
	



3.1.216.1790 – 4/10/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	Dev - EMV 3.1: Log Dispenser Blend Ratios for DXMonitor (Request from Casey's and Murphy USA)
	X
	X
	X

	EMV 3.1: Screen hangs on "wait for scd ready" on Jadescd setup during and after installation of 3.1.215.1750 via Service Utility
	
	
	X

	EMV 3.1 Anthem: Credit/Debit/Pay_Inside visible when COIPA
	X
	
	



3.1.215.1750 – 3/24/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: Soft Key are not removed from the screen when a card inserted, started happening in 3.1.212.1130
	
	X
	

	EMV 3.1: 3.1.215.1670 Jade\SCD - Fails to install and run.
	
	
	X



3.1.215.1730 – 3/12/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1:  SPM2.5 - Shell Canada - SPM/POS Communication - NCR - RPOS 2023.1.10
	X
	X
	X

	EMV 3.1 Anthem: Logic issue in pairing system.config updates
	X
	
	



3.1.215.1670 – 3/3/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: Visa Fleet Test Case 8008b Contactless Tap Returns no data or missing Fleet data
New Contactless Middleware:  3.1.0.56
	X
	X
	X

	EMV 3.1: Card reader non responsive on SPM2.5r after a period of idle
New SPM2.5R OS from XAC:  250221
	X
	X
	

	Dev - EMV 3.1: Merge SPM2.5e Fixes from 2.8->3.1
	X
	X
	X

	Changes from XAC to accommodate TR34 for RKI
SCD OS:  240514
SCD2.5 OS: 250116
SCD Firmware: 240619
	
	
	X




3.1.215.1660 – 2/13/2025

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1.214: EMV Language Prompt Crashes if Unchanged
	X
	X
	X



3.1.215.1650 – 1/30/2024

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: KeypadFunctionKeys values being returned different on Anthem vs 2.8 when Cancel is Clear Enabled.
	X
	X
	X

	EMV 3.1:   SCD serial number and SCD OS version are not logged to asset manager log
	
	
	X



3.1.215.1620 – 1/7/2024

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	SPM2.5R: Remote Upgrade Modifications
	X
	X
	



3.1.215.1600 – 1/3/2024

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	Anthem: Latest SPM2.5R FW, Latest SPM2.5R OS not included in latest build, for example 3.1.214.1470 at 16 Oct 22:01
SPM2.5R OS              241101
SPM2.5R Firmware            240716
	X
	X
	

	EMV 3.1: New SPM2.5\SPM2.5R OS\FW from XAC to Fix "WDT Not Restarting CPU"
	X
	X
	



3.1.215.1590 – 12/11/2024

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 New Terminal Protocol Command\Response for Anthem Third Party Data (e.g. Loyalty)
	X
	X
	X



3.1.214.1560 – 12/6/2024

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: Card App Preferred Language Not Triggering CurrentLanguageChanged Event - Interac03 Test Case
	X
	X
	X

	EMV 3.1: P2PE BIN Table Remote Update via DXMonitor (Investigate and Scope) [WCrypto, DFSKPT, WRSA]
	X
	X
	X



3.1.214.1540 – 11/25/2024

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: TLS Handshaking is out of sequence and can cause connection issues.
	X
	X
	X



3.1.214.1530 – 11/20/2024

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV3.1 – Non-Responsive - Murphy 8637 T7 DEF
SDVM T7 OS 231108
	
	X
	

	EMV 3.1: Jade\SCD - SPM2/SPM2.5 OS/FW is provided to SCD/SCD2.5
	
	
	X

	EMV 3.1:  T7\T12\Anthem - SPM2/SPM2.5 OS/FW is missing FW
	
	X
	

	EMV 3.1: Modify GetDeviceManufacturerCommand to Specify Anthem
	X
	
	



3.1.214.1520 – 11/8/2024

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 Anthem: COIPA - Chevron - Anthem – Verifone
SPM2    OS 230706
SPM2.5 OS 241015
	X
	X
	



3.1.214.1510 – 11/7/2024

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 (Anthem): Need the Printer to advance the Paper during the upgrade process on the SPM
AutoUpdateEU_Anthem 1.0.2.73
	X
	
	

	EMV 3.1 Anthem: COIPA - Chevron - Anthem – Verifone
SPM2 OS 20230706
	X
	
	



3.1.214.1500 – 11/5/2024

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: Anthem: At restart time, system is restarting an extra time because of timezone setting
	X
	
	

	EMV 3.1: Performing "Get Display Command" shows IsColor=false
	X
	
	

	SPM2.5R Fails to Pair with Anthem after update.
Needs new SPM2.5R OS:  241101
	X
	
	



3.1.214.1470 – 10/16/2024

	Description

	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: Walmart production beta issue - MSR transactions
	X
	X
	

	EMV 3.1: Interac Contact Test Case Inter03 Fails
	X
	
	

	EMV3.1: SCD OS version, and other HW data is logged as empty
	X
	X
	X

	EMV 3.1: Transition to operational mode must not be allowed if secure module maintenance mode key is not injected
	X
	X
	X



3.1.214.1420 – 9/23/2024

	Description

	Anthem
	T7/ECIM
	Jade+SCD


	EMV 3.1.212: Flash Space Reporting Incorrect
	X
	X
	

	SPM2.5R: Suppress Compressed Logging for Anthem when SPM2.5R Installed
	X
	
	

	EMV 3.1: WCrypto P2PE BIN Table & Config File Update Via Service Utility (SU)
	
	X
	X



3.1.213.1390 – 9/4/2024

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: Interac Contact Test Case Function02 Fails (works on EMV 2.8) - For Bulloch
	X
	X
	X

	EMV 3.1 Anthem: COIPIA: PCI restart request fails to stop WDT
	X
	
	

	EMV 3.1 Anthem: Flashing texts in a language other than English
	X
	
	

	SPM2.5R: Anthem AutoUpdater (AU)
· Version 1.0.2.72 EU AU
	X
	X
	

	SPM2.5R: Domestic AutoUpdater (AU)
	X
	X
	

	SPM2.5R: Service Utility Modifications
	X
	X
	



3.1.213.1340 – 8/9/2024

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: Transition to operational mode must not be allowed if secure module maintenance mode key is not injected
	X
	X
	X

	EMV 3.1.213: Open Architecture - KeyPressed event with full ZIP data is sent twice
	X
	
	



3.1.213.1320 – 7/1/2024

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 Remote update fails when the terminal Secure params files are included in the CAB
	
	
	X

	EMV 3.1 Open Architecture: EMV 3.1.213 - Implement New Command\Response During EMV PIN Entry to denote that User has Selected PIN Bypass or Cancel Softkey
	X
	
	

	EMV 3.1 Open Architecture: Request for GetTimeCommand and GetSoftwareStateCommand doesn't return properly
	X
	
	

	EMV 3.1 Open Architecture: Request for ChallengeCode returns a valid code BUT Success="false" all the time
	X
	
	

	EMV 3.1 Open Architecture: EMV 3.1.213 - Add Secure Prompt ID To the EMVModuleStatusChanged Event for EMVModuleState="EnterPIN"
	X
	
	






3.1.213.1230 – 6/12/2024

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 [Anthem] [SPM2]: While in Maintenance mode the Diagnostic Card Reader test failed to read Chip card
	X
	
	

	EMV 3.1 (Anthem): Change the SPM behavior to block SPM System Clock updates for when the date is not within the valid SSL certificate dates to prevent loss of communication with the POS
	X
	
	

	SPM2.5R: Integration Iterations with XAC
· adds SPM2.5R board type and logic, removes display recovery hack, and SPM2 barberpole hack
	X
	X
	

	EMV 3.1: Terminal OperationalStatus Not Updating With EMV App/Keys
	X
	X
	X

	EMV 3.1: Updating IGEM when the Printer is offline , the error message in DX monitor says "Invalid download - component not upgradeable"
	X
	X
	X

	EMV 3.1 Open Architecture: EMV 3.1.213 - Send Prompt Text with DisplaySecurePromptResponse
	X
	
	

	EMV 3.1 Open Architecture: EMV 3.1.213 - Add New Configuration Option isOpenArchConfiguration
	X
	
	

	EMV 3.1 Open Architecture: EMV 3.1.213 - During EMV PIN Entry, Send KeyPressed and PINEntryComplete Events
	X
	
	

	EMV 3.1 Anthem:  Keypad function keys are losing their definitions.
· keypad/functionkeys were disabled after DisplayPromptCommand
	X
	X
	X



3.1.212.1130 – 5/23/2024

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 Anthem:  Keypad function keys are losing their definitions.
· keypad/functionkeys were disabled after DisplayPromptCommand
	X
	X
	X



3.1.212.1120 – 5/15/2024

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 (Anthem): Woodland ARCO upgrade failed due to SVMX reset request just prior to FileReplication.
	X
	
	

	EMV 3.1 Anthem:  Keypad function keys are losing their definitions.
· Needed for MurphyUSA
· Note to QA:  need to test Anthem, T7 and Jade\SCD
	X
	
	





3.1.212.1100 – 4/18/2024

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 (Anthem): EMV is sending clear soft keys flag always set to false
	X
	
	



3.1.212.1090 – 4/10/2024

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: T7 Service Utility Upgrade Crash on Restart
	X
	X
	X

	EMV 3.1: SU Upgrade for DS457 scanner  newer model fails on Jade/SCD
	
	
	X



3.1.212.1070 – 03/26/24

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 (Anthem): add flash space RemoteMessage to allow SVMX/DXMonitor to alert low flash space condition
	X
	
	

	EMV 3.1: Verify the Zebra Release FW for new T7 Scanner
2D: Zebra PL5000 
•          Firmware CAAEOS00-004-R01D0
	X
	X
	X



3.1.212.1050 – 03/25/24

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 P2PE: Component 180 requires Secure Prompts to be included in the CAB file for remote upgrades.
	
	X
	X

	EMV 3.1 Anthem: FileReplication module maps both C150S and C150SE folder into C150FW folder.
	X
	
	

	EMV3.1 Anthem SPM2.5 Firmware update package installs Contactless package that leave it in a FirmwareUpdating state. Not readily recoverable
	X
	
	



3.1.212.980 – 2/13/2024                                                                       

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1.212: Set Tag 9F0C in Brand Application Volatile Data on WayneTap
	X
	X
	X

	EMV 3.1 Anthem: DisplayPrompt IgnoreSoftKeySet="true" is Ignored
	X
	
	

	EMV 3.1 (Anthem): Send SVMX Board the POS Display Images and POS Display Prompts
	X
	
	

	EMV 3.1: Anthem AU V 1.0.2.64 fails to install when running from USB stick
	X
	
	



3.1.211.950 – 2/1/2024

	[bookmark: _Hlk158796286]Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 Anthem Remote Update: AutoUpdate processes compressed binaries
	X
	
	

	EMV 3.1.211: EMV Contactless C150SE Firmware with Old Kernels
	X
	X
	X

	EMV 3.1.211: EMV Contactless C150SE Firmware to Return Tag 9F0C (Issuer Identification Number Extended)
	X
	X
	X

	EMV 3.1: System is not sending a ResetPending Operational Status to POS before Nightly Reboot.
	X
	
	

	EMV 3.1 Default Security Setting seems to be wrong for DXMonitor
	
	X
	X

	EMV 3.1: L ERROR - OnProcessAPDUResult - Insufficient buffer! resulting in an F201 Error
	X
	X
	X

	EMV 3.1.210: Remote update for WayneTap (C150S) Peripheral Device f/w via DXM on Anthem - QA
	X
	
	

	EMV 3.1 (Anthem) - Serial Printer is not working with Anthem
	X
	
	

	EMV 3.1 Anthem Remote Update: AutoUpdate processes compressed binaries
	X
	
	

	EMV 3.1: Anthem AU V 1.0.2.64 fails to install when running from USB stick
	X
	
	

	EMV 3.1 P2PE App presents unhandled domain exception
	X
	X
	X

	EMV 3.1 Anthem Remote Update: Compressed updates issue in FW updates, Application updates
	X
	
	

	EMV 3.1 Anthem: Temp files cleanup crashes SPM2
	X
	
	

	EMV 3.1: Soft key pressed detail is incorrect in SPM2.txt (functionality is correct, logging key is not)
	X
	X
	



3.1.211.920 – 12/6/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: Anthem AU V 1.0.2.64 fails to install when running from USB stick
	X
	
	

	EMV 3.1 P2PE App presents unhandled domain exception
	X
	X
	X



3.1.211.900 – 12/1/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 Anthem Remote Update: AutoUpdate processes compressed binaries
	X
	
	



3.1.211.890 – 11/30/2023

	[bookmark: _Hlk158796173]Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 (Anthem) - Serial Printer is not working with Anthem
	X
	
	



3.1.211.880 – 11/17/2023

	[bookmark: _Hlk158792725]Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 Anthem Remote Update: AutoUpdate processes compressed binaries
	X
	
	

	EMV 3.1.211: EMV Contactless C150SE Firmware with Old Kernels
	X
	X
	X

	EMV 3.1.211: EMV Contactless C150SE Firmware to Return Tag 9F0C (Issuer Identification Number Extended)
	X
	X
	X

	EMV 3.1: System is not sending a ResetPending Operational Status to POS before Nightly Reboot.
	X
	
	

	EMV 3.1 Default Security Setting seems to be wrong for DXMonitor
	
	X
	X

	EMV 3.1: L ERROR - OnProcessAPDUResult - Insufficient buffer! resulting in an F201 Error
	X
	X
	X

	EMV 3.1.210: Remote update for WayneTap (C150S) Peripheral Device f/w via DXM on Anthem - QA
	X
	
	




3.1.210.790 – 10/09/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 – Configuration receipt missing top 5 sections of the receipt
	
	
	X

	EMV 3.1(DFSKPT – ACI):Encryption format is incorrect for the chip cards set in whitelist to mask PAN only.
	X
	X
	X








3.1.210.770 – 9/29/2023
	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: Unhandled domain exception in DisplayController startup creates race and crash at startup.
	
	
	X

	EMV 3.1 Anthem Remote Update: consolidate versions reporting
	X
	
	

	EMV 3.1 (Anthem): SPM2 should Reboot when Terminal is Idle (or wait a max of 30 mins)
	X
	
	



3.1.210.740 – 9/21/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 Jade\SCD: System hangs after a reboot when system is configured for iXMedia with no Edge Box attached.
· Modified iSense.heartBeatInterval from 5 to 29 secs in System.config files
	
	X
	X

	EMV 3.1.210: Remote update for WayneTap (C150S) Peripheral Device f/w via DXM on Anthem – Development
· delete card reader and tap reader FW folders at FR time
	X
	
	



3.1.210.720 – 9/15/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: DFSKPT P2PE Enhancement for GlobalPayments (Contact) 
	X
	X
	X

	EMV 3.1: DFSKPT P2PE Enhancement for GlobalPayments (Contactless)
	X
	X
	X

	EMV 3.1.211: Return Tag 9F0C (Issuer Identification Number Extended) in ApplicatonSelected Event and AIDCandidates Event
	X
	X
	X

	EMV 3.1.210: Remote update for WayneTap (C150S) Peripheral Device f/w via DXM on Anthem - Development
	X
	
	

	EMV 3.1: Mag Card Reader Type needs to report as "Swipe" and not Insert to follow 2.8.
	X
	X
	X

	EMV 3.1: SetPromptID does not allow promptID="0" as 2.8 does.
	X
	X
	X

	EMV 3.1.209: ResetDHCP request requires a minimal number of parameters on the TLV data:
· Fixed issue that SPM IP is cached, and pairing heartbeat is informing the old IP, when the DHCP server assigns a new IP
	X
	
	





3.1.210.640 – 8/31/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: DF30, DF32 for Fleet is not reporting in the ApplicationSelected portion of the transaction when tags are enabled for that section
	X
	X
	X

	EMV 3.1 (Anthem): Substitute Command is not working (A12)
	X
	
	



3.1.210.620 – 8/22/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 (Anthem): SPM2 Pairing information not correctly stored to the config file when DHCP is enabled.
	X
	
	

	EMV 3.1.209: T7 scanner support for Jade/SCD
	
	
	X

	EMV 3.1.209: SU Upgrade for T7 Scanner on Jade/SCD
	
	
	X



3.1.210.600 – 8/09/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1.210: New Contact EMV Kernel DLLs from XAC to Fix 2 Test Cases
	X
	X
	X



3.1.210.590 – 8/01/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: Path in nativecertificates validator is wrong (bclib.dll not deleted by payment app correctly)
	X
	
	

	EMV 3.1 date time format on Jade/SCD startup splash needs to be shortened
	
	
	X

	EMV 3.1.209: ResetDHCP request requires a minimal number of parameters on the TLV data:
	X
	
	

	EMV 3.1.210: New Contact EMV Kernel DLLs from XAC to Fix 2 Test Cases
	X
	X
	X



3.1.209.550 – 7/21/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV3.1(Jade/SCD) - Full software Remote upgrade using DX Monitor causing dispenser to reboot after every 5 minutes after the successful upgrade
	
	
	X

	EMV 3.1.209: ResetDHCP request requires a minimal number of parameters on the TLV data
	X
	
	



3.1.209.520 – 7/18/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 - P2PE : ACI/ABSCO - Volatile block is formatted incorrectly
	X
	X
	X

	EMV 3.1: L ERROR - OnProcessAPDUResult - Insufficient buffer! resulting in an F201 Error
	X
	X
	X



3.1.209.500 – 6/15/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 (Jade/SCD) - Prompt file is missing from SU (DefaultPrompts.config)
	
	
	X

	EMV3.1 Service Utility - Fix the usage of files in /flash/ which is causing locking issues
	
	
	X

	EMV 3.1 Jade\SCD: Get Serial Number of P90 CR on a Jade platform.
	
	
	X



3.1.209.480 – 6/15/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 (Jade/SCD) - Prompt file is missing from SU (DefaultPrompts.config)
	
	
	X

	EMV 3.1 Jade\SCD: Get Serial Number of P90 CR on a Jade platform.
	
	
	X



3.1.209.470 – 6/12/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: IXPay2 - Failed to send SecurePrompt ID "1008" Entered Amount Over Limit when entering over Preset Amount
	X
	X
	X

	EMV 3.1: Anthem's DisplaySecurePrompt MinLength Not Functional
	X
	
	

	EMV 3.1: P2PE Bin Range 600315 is not providing P2PE Data, Bin File attached.
	X
	X
	X

	EMV 3.1.209: SCD Startup Progress on Display
	
	
	X

	EMV 3.1 Jade\SCD:  Readers are not coming online after a reboot randomly
	
	
	X





3.1.209.430 – 6/01/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1 Jade\SCD:  Readers are not coming online after a reboot randomly
	
	
	X



3.1.209.390 – 5/22/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1.209: No POS Reconnect after SPM Ethernet Disconnect
	X
	
	

	EMV3.1: CAT improperly protected in critical chip EMV phases - display (QuickChip)
	X
	X
	X

	EMV 3.1.209: IXPay Test Tool does not saved its own saved scripts, they need to be modified to remove carriage returns to make a single line
	X
	X
	X

	EMV 3.1: In contactless PIN entry, pressing clear on empty buffer improperly disables keypad entry
	X
	X
	X



3.1.209.390 – 5/22/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1.209: No POS Reconnect after SPM Ethernet Disconnect
	X
	
	

	EMV3.1: CAT improperly protected in critical chip EMV phases - display (QuickChip)
	X
	X
	X

	EMV 3.1.209: IXPay Test Tool does not saved its own saved scripts, they need to be modified to remove carriage returns to make a single line
	X
	X
	X

	EMV 3.1: In contactless PIN entry, pressing clear on empty buffer improperly disables keypad entry
	X
	X
	X



3.1.209.320 – 4/28/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1.209: No POS Reconnect after SPM Ethernet Disconnect
	X
	
	

	EMV3.1: CAT improperly protected in critical chip EMV phases - display (QuickChip)
	X
	X
	X

	EMV 3.1.209: IXPay Test Tool does not saved its own saved scripts, they need to be modified to remove carriage returns to make a single line
	X
	X
	X

	EMV 3.1: In contactless PIN entry, pressing clear on empty buffer improperly disables keypad entry
	X
	X
	X



3.1.208.240 – 4/12/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: Getting a softkey type selection on a T7 after installing 3.1.208.180 release
	
	X
	



3.1.208.180 – 3/23/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	IXEMV3.1(DFSKPT - CircleK) - PAN is sent in clear text exposing tag57 for chip cards set in whitelist to mask PAN only
	X
	X
	X

	DFSKPT ACI Specific p2pe.config file
	X
	X
	X


[bookmark: _Hlk130487777]
3.1.208.170 – 3/20/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: Service Utility issues during ABSCO/DFSKPT installation style update of production signed instance
	
	X
	X

	EMV 3.1.208: Smart Remote Upgrade Functionality (SCD/SCD2.5)
	
	
	X

	EMV 3.1.208: Smart Remote Upgrade Functionality (P90/P95/Sankyo Cardreaders)
	
	X
	

	EMV 3.1: Card Reader AutoLock default should be set to "true".
	
	X
	X

	EMV 3.1.208: Test New Jade OS 6.xx.113 that fixes Jade Field Issues 
New Jade OS 6.XX.113 to address “Flash Corruption” and “No Heartbeat” field issues with Jade
· Fix: Jade board had an issue during power ON, where the eMMC controller had a bad power of around 2 Volts for ~12mSecs, which could cause the Jade to not start properly (no heartbeat) or could cause flash data corruption. This window of the eMMC controller without proper power      increased when the SW Reset via PMIC was introduced in Jade OS 6.XX.110. Jade OS 6.XX.113 will provide the SW workaround for the issue, and a final fix would be to re-work the power rails of Jade in next releases of the HW.  See attached notes and PPT slides for more details.
	
	
	X

	EMV 3.1:  Persisted data is missing from the P2PE block for Contactless EMV card only (DFSKPT ACI)
	X
	X
	X

	EMV3.1 (DFSKPT): When P2PE is disabled, P2PE datablock is sent for Magstripe data events
	X
	X
	X



3.1.208.110 – 3/14/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1.208: Keypad Function Keys - Support for Anthem
	X
	
	

	EMV 3.1.208: Provide the P2PE data blob for the whitelisted transactions when P2PE provider is ACI
Added default P2PE config for ACI
	X
	X
	X



3.1.207.570 – 2/16/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1.207: Smart Remote Upgrade Functionality (SPM2/2.5)
	
	X
	

	EMV 3.1: Soft Key selection screen appears to be hard coded and the right side soft keys are not enabled for this prompt.
	
	
	X



3.1.207.570 – 2/16/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1.207: Smart Remote Upgrade Functionality (SPM2/2.5)
	
	X
	

	EMV 3.1: Soft Key selection screen appears to be hard coded and the right side soft keys are not enabled for this prompt.
	
	
	X



3.1.207.550 – 2/16/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: DFSKPT ACI Block Format EMV tags inclusion
	X
	X
	X



3.1.207.530 – 2/07/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1.207: Heartbeat counter is only started after the first Heartbeat response and only resets the counter on Heartbeat Messages
TCP and TLS improvements
	X
	X
	X

	EMV 3.1: Service Utility issues during ABSCO/DFSKPT installation style update of production signed instance
	
	X
	X

	EMV 3.1: Service Utility Does Not Display Contactless Reader FW Update
	
	X
	X

	EMV 3.1.207: SPM2.5e - Retrieve Logs via Service Utility
	
	
	X

	EMV 3.1: ContactKernelVersionInformation does not display when Sending Command with the IXPay Test server version 3.1.205.57
	X
	
	

	EMV 3.1.208: Enable 'IPCONFIG release\renew' once triggered from Anthem
	X
	
	



3.1.207.430 – 1/11/2023

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1.207: Service Utility should handle FW upgrade for SPM2.5e vs SPM1 for Jade/SCD
	
	
	X

	EMV 3.1.207: Remote FW upgrade for SPM2.5e vs SPM1 for Jade/SCD
	
	
	X

	EMV 3.1.207: DFSKPT P2PE Enhancement for DFS P2PE Customer ABSCO with Provider ACI
	X
	X
	X



3.1.207.410 – 12/05/2022

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1.207: SPM2.5e - Retrieve logs remotely
	X
	X
	X

	EMV 3.1.207: DFSKPT P2PE Enhancement for DFS P2PE Customer ABSCO with Provider ACI
· Added TLV format for ACI EMV chip card and EMV chip encryptions modified to be binary not ASCII
· Encrypt data function returns byte array instead of base 64 string
	X
	X
	X

	EMV 3.1: Canada transaction failed to display Account Type Selection, "EMVKernelController L ERROR - Account Type Selection timed out or cancelled"
	X
	
	

	EMV 3.1.207:  Heartbeat counter is only started after the first Heartbeat response and only resets the counter on Heartbeat Messages
	X
	X
	X

	EMV 3.1: (Anthem) - Dispensers not reading cards
	X
	X
	X

	New Jade OS 6.XX.112 (for iXPay SPM2.5 Device Upgrade features):
· Upgrading 2D Bar Code scanner firmware (via Service Utility or Remote Upgrade) fails due to serial emulation issue (bytes are dropped when buffer is full – exposed with faster processor of iXPay SPM2.5)
· Fixed issue with the SPM Driver, where the emulation layer was dropping bytes with the SPM2.5e
· Works in conjunction with iXPay SPM2.5 version 2.2.81 and later to fix upgrade of serial devices (barcode scanner and chip card reader)
	
	
	X



3.1.207.330 – 11/03/2022

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1: (Jade/SCD - DFSKPT) - Download File command is not working with the whitelist
	X
	X
	X

	EMV 3.1: CTLS Status Not Checked Before Attempting OpenReader
	X
	X
	X

	EMV 3.1.207: Investigate Timing for Shell\VF Anthem v. EMV 2.8
	X
	
	

	EMV 3.1: Transaction Aborts immediately instead of Retrying after Set Amount exceeds maximum amounts. Expectation is it should retry Set Amount
	X
	X
	X

	EMV 3.1: (Jade/SCD - DFSKPT) - Magstripe only cards payload is not in the ACI block format
	X
	X
	X

	EMV 3.1: Anthem Canada, First Debit Transaction each day fails
NOTE:  this requires new SPM2.5 OS to store MSM Working Keys in Flash as opposed to RAM
	X
	X
	

	EMV 3.1.207: Add SPM2.5 OS 20221020 to BB fix Working Keys Not Persistent Across Reboot
	X
	X
	



3.1.207.290 – 10/21/2022

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	DFSKPT P2PE Enhancement for DFS P2PE Customer ABSCO with Provider ACI.
	X
	X
	X

	EMV 3.1 DFSKPT and WRSA whitelist processing fails intermittently on larger whitelists
	X
	X
	X

	EMV 3.1.207: SPM2.5e - Retrieve Logs via Service Utility
	
	
	X

	EMV 3.1: VerifyMAC() issue for SPM2\SPM2.5
Merged from EMV 3.1.205
	X
	X
	

	EMV 3.1.207: Autoupdator changes to handle new Scanner FW upgrade
	X
	X
	

	EMV 3.1.207: Upgrade functionality for multiple device configurations via Service Utility or Remote Upgrade
	X
	X
	X

	EMV 3.1.207: Verify the Zebra Release FW for new T7 Scanner
	X
	X
	









3.1.207.250 – 10/7/2022

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1.206: Fallback from DHCP to last known good Static IP address (Merge from EMV 2.8.206)
	X
	X
	X

	EMV 3.1.206: T7 - Verify Scanner Firmware versions before local and remote FW upgrades
	X
	X
	

	EMV 3.1.206: Add Zebra Firmware for new HW PL5000 Unit (T7 and Anthem Only)
	X
	X
	

	EMV 3.1.206: T7 Service Utility - Upgrade time needs to be increased
	
	X
	

	EMV 3.1.207: Autoupdator changes to handle new Scanner FW upgrade
	X
	X
	

	EMV 3.1.207: Upgrade functionality for multiple device configurations via Service Utility or Remote Upgrade
	X
	X
	X

	EMV 3.1.207: Verify the Zebra Release FW for new T7 Scanner
	X
	X
	

	Add Teamcity Support for Remote Upgrade for Production Anthem MSIs
	X
	
	

	EMV 3.1: Anthem EMVKernelConfiguration.xml is missing attributes.
	X
	
	

	Anthem fails to display the Decimal point in the Secure prompt $% value $15000. It should be $150.00 or just $150
	X
	
	

	EMV 3.1: MasterCardPromptscriptfileHandler error
	X
	X
	X

	EMV 3.1: Intermittent Secure Prompts / POS Race Condition
	X
	X
	X

	EMV 3.1 (Anthem): Keypad Format Exception Error
	X
	
	



3.1.205.70 – 12/17/2021

	Description
	Anthem
	T7/ECIM
	Jade+SCD

	Anthem: C150S Contactless card readers on SPM2.5 not completing upgrade of FW for Anthem dispenser
	X
	
	

	EMV 3.1.204: Media is enabled when touchscreen alphanumeric keypad is visible
	
	X
	

	EMV 3.1.204: TouchScreen AlphaNumeric keypad is visible when the terminal is set to idle and EO1 prompt is displayed
	
	X
	

	EMV 3.1 Jade/SCD/SPM1 is in init mode, CANCEL at AccessControl blanks the display
	
	
	X

	EMV 3.1 - Data entry complete event is suppressed when touch and phy keypads both enabled
	X
	X
	

	Anthem: Dynamic prompts not working on boot after install
	X
	
	

	Anthem: WPF.977 message on the screen after install of 1.14 on fresh OS
	X
	
	

	EMV 3.1 Media play obscures T7 Access Control if touch keypad configuration is set
	
	X
	



3.1.205.10 – 12/05/2021

	[bookmark: _Hlk158799233]Description
	Anthem
	T7/ECIM
	Jade+SCD

	EMV 3.1.205:  Visa EMV Fleet 2.0 Implementation (Contact)
	X
	X
	X

	EMV 3.1.205: Implement Voyager EMV Prompt Script File
	X
	X
	X

	EMV 3.1: FunctionKey Navigation for Anthem Helix ADA
	X
	
	

	EMV 3.1.205: P2PE on Anthem - Default Config Files
	X
	X
	X

	EMV 3.1 T7 Missing Config file for DFSKPT P2PE from SPM2/IxPaymain
	X
	X
	X
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