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North America Anthem Release Notes

1.24.2 – 08/05 2025

1. Fix for displaying DriverID secure prompt.
1. Fix for flow rates reporting foe AX12.
1. Prompt mapping enhancements.
1. Anthem time synchronization enhancements.

1.24.2 – 05/08 2025

· Additional integration with Bulloch POS
· Additional Canada Market integration
· Introduced DFS SaaS team feature to remotely configure fuel product assignments.  
· Welcome text is now configurable in Application Settings by ASO and remote DFS SaaS.
· Smiley face can now be replaced with retailer logo with a branding pack request.
· Improved SW Update screen on Anthem so it is very apparent that an update is in progress.  The message asks to wait and NOT interrupt power.
· Removed guidance text in footer.
· Re-work media integration for DX Promote Auto
· Added time sync button to force time sync.
· Improved Verifone loyalty prompt integration
· Improved Aurus integration
· Improved Allied integration.
· Improved Fiscal integration.
· Enhanced the iGEM 2.5 integration.
· If NCR RPOS, Minimum version is 

1.24.0 – 03/18 2025

· Remove 'Next Step' from prompting.
· Display media directly from anthem.
· Add RabbitMQ logs to SVMX logs.
· iGem2.5 - update job names for igem2.5 in DXM.
· Display ATC compensation message with translation.
· Remote product assignment.
· Updated package for Gilbarco, which include updated secure prompt files.
· Accept default EMV configuration per POS.
· Create a POS vendor with configs for Midax.
· Pass grade information with flow rate to DXM.
· Display banner with loyalty content for Bulloch POS.
· Move all install MSI into SVMX core.
· Update Electron version in Display app.
· Add Caseys prompt mapping.
· Secure prompts change for Anthem for Allied.
· Pump controller to pick iGem version.
· Display upgrade status for iGem2.
· Enable displaying images in passthrough.
· Need to add Prompt mapping Rule to handle when an ImageId is added to SetPromptDetailsCommand.
· Combine Help modules into one.
· Send dispenser information to POS.
· Update endpoint list for Installation wizard.
· Pump controller to run in idle mode.
· Automatic time sync - add Sync button.
· Combine iGem1.5 and iGem2.5 plugins.
· iGem 2.5 - Send flow rates to DXM.
· Use NTPServer URL from approved firewall policy list.
· Add possibility to display SVG graphics.
· Welcome text is customer editable.
· Send idle alert to DXM.
· Please Standardize the DX Promote Media Settings.
· To add CAN FW Version to DXM.
· SAM to display install status.
· Anthem 1.23: Maintenance Softkeys Unresponsive (regression?)
· PumpController stopped working after changing date & time settings.
· Grade configuration view skipped during Load Template process.
· DX Configuration POS Prompt Variant not showing variants.
· Anthem 1.24: Anomalous DisplayPrompt Behavior.
· SPM enters maintenance mode after automatic date & time settings change.
· Pump grades don't save during first loading template.
· Installation wizard shuts down unexpectedly during grade configuration.
· Printer telemetry issue when printer not connected.
· While doing back-to-back sessions on TU1 post2, I noticed that if I let the end of session “do you want a receipt” screen to timeout, the next sessions data would remain on the graph.
· Using MAC address for Anthem-SPM connection causes connection drop.
· LEM meter API used too often.
· Anthem 1.23.4: Date/Time Softkey Stall.
· Anthem 1.23.5: iSense Drop / Screen Freeze.
· Branding pack uninstalled/removed after SAM upgrade with |ERROR|ApplicationInfoService|Error while enumerating installed app: 'SVMX.CustomerAppUIBrand W2894310-002-07_WayneGeneric'.
· Factory Restore failed to recover corrupted install ERRORs. ApplicationInfoService|Error while enumerating installed app: 'SVMX.Plugins.PumpController.IGem.Base'.
· DXP Media set rendering issue when uploading ultra-wide videos. Causes the Media panel to expand unexpectedly.
· POST number displayed twice in the maintenance main screen.
· Printer not connected.
· DXP Shows Terminal Status as Offline on Version 1.24.0.723.
· EMV Function keys not detected in Diagnostics Keypad Test after transaction.
· Installation wizard do not enter to “Apply Configuration Parameters” return OoS.
· HostedApps preview missing 'back' button.
· 3rd party apps not loading.
· Anthem Help panel do not react to Close button.
· Pax configuration doesn't save when instance,evCharger,pax.configurations files was selected.
· Smart Security Switch Plugin is not starting.
· Wet test section returns an empty field on AX7 and AX12.
· Meijer Anthem Reverts to White Mode Display After Switching to Dark Mode During End-to-End Transaction.
· LED - DIM option not staying after leaving from anthem screen.
· Anthem writing 1.6 client config to longship, need to disable it.
· RFID- Reader doesn’t show up the content while tapping the RFID Card.
· After cloning configuration from liteboard to AX27, can't change Network Interface.
· Installation wizard freezes on Date & Time setup.
· LEDs not changing color at Spatco.
· Date & Time Setup return to IDLE when incorrect year value applied.
· Anthem 1.23: Hosted Apps Preview Stall w/ Tier 0.
· After clicking on Hosted Apps Preview, the system stops responding.
· Date set to year 1900.
· Logging time malfunctioning after changing the time zone.
· CustomerAppUI stopped. ENTER LOYALTY ID secure prompt screen frozen. Reboot Anthem required.
· File distribution update status is incorrect.
· DXM flow rate issues with 1.22.3 update.
· Software sharing blocked by iGem plugins merge.
· incorrect thirdpartyapps new button header/label.
· Tier's hash is not created after full installation.
· After saving configuration maintenance menu is closing.
· File distribution failure - checksum mismatch.
· Validation of .net version before SAM installation.
· Branding test reports malfunction.
· Touch malfunction during configuration.
· Repetitious changing the language triggers the maintenance screen.
· ANTX WIN10IOT can boot into recovery (WinRE) allowing access to file system.
· Incorrect positioning of grades

1.23.0 – 08/30/2024

· Custom Prompt Mapping for Verifone JumpStart 1.23 pilot week of 9/16
· Add InfoNet configuration for Canada Pilot with EMVKernelConfiguration.xml, and Secure Prompts, Pilot date is Monday Sept 16, 2024
· iGem 2.5 - Calibration and ATC Mode screen modifications
· Infactory mode - notification if tiering is installed.
· Display configuration and diagnostics options based on peripherals' availability.
· Add support for zip in SAM.
· Incorporate Custom Prompt maps in config default.
· Pass phone number to 3rd party app.
· 3rd party apps to display media content.
· Revert pre-fueling panels for ADA.
· Installation wizard - site connection
· Installation wizard - add SPM replication statuses.
· ConfigurationChangeLog to reflect CM changes.
· Remove sync SPM setup.
· Update time zone description
· Prepare Anthem OS image.
· iGem2.5 - disable door security.
· Do not display language selection in passthrough.
· Installation wizard - expand a template list.
· Add QR code for edge network tool.
· PIN mask to be displayed only after key pressed.
· Installation wizard - POC adapt edge network tool to wizard.
· Installation wizard - Add date time screen.
· Installation wizard - Display site linking error.
· Installation wizard - network connectivity screen updates
· Enable rebooting SPM from DX Monitor
· iGem2.5 - Fuel Theft warning message
· iGem2.5 - Anthem displays W&M info when CRC button on iGem board is pressed.
· iGem2.5 - Anthem adds floating keypad (a.k.a. IR Remote Control) when product buttons are shown in diagnostic mode.
· Enable auto linking directly through IoT hub.
· Installation wizard – flow.
· Installation wizard - UI adjustments for AX7 and AX12.
· Installation wizard - settings screen.
· Installation wizard - SPM configuration screens.
· Possible to select template file from dispenser level.
· Installation wizard – prerequisites.
· Installation wizard - pump configuration screens.
· Installation wizard - network connectivity statuses.
· Ready state of charge showed up in Anthem while ECOG is not ready.
· Flashing texts in a language other than English.
· Invalid JSON format, should not have a comma at the end of "DefaultCustomerName": "to Marathon!",
· LEDs not working consistently.
· 'Time remaining' displays incorrect values.
· SAM starts remote software update when charging is in progress.
· Emergency Stop from car , NOT showing up and not able to disconnect the cable from car
· Display only 3 digits of KW used in the receipt.
· Invalid configuration_*.zip installation on EVC.
· 'Disable door security' job not working on pump side B.
· 1.22.3: Copy Tiering Nonfunctional.
· Anthem does not show CLOSED LOCK icon when door-security ARMED.
· Cannot set properties of null (setting 'MediaWidth').
· As a parameter header appears 'root'.
· ANT Board losing the FP address FP#2 CANBUS.
· AX12 - During Fueling many ERRORs reported, |ERROR|Image error {"isTrusted":true} (https://127.0.0.1:5000/main.7bf0312b72126155.js:1).
· When post is unavailable, transaction should be terminated.
· 1.22: RemoteMessage GetLanguageName Not Answered.
· iGem2.5 - Improper door security alarm displayed in DMX.
· CPMS status incorrectly showed.
· Up on clicking CLOSE button - EV Charging showed " Please Wait" but actually didn’t stop the session.
· EVC - Software distribution between dispenser’s malfunctions.
· iGem2.5 - Anthem takes up to 1 second instead of 1 or 2ms to respond to CAN remote frame.
· iGem2.5 - Anthem sends a series of ACKs to sales data instead of one at a time.
· 1.23: PumpController / TSM Not Respecting No/External Pump Mode.
· Installation wizard - template issues.
· DXM is missing flow rate data from Anthem boards.
· User gets kicked to the main screen during printer diagnostics.
· Dispenser stuck on 'Pay the clerk inside' after installation on cleaned up device.
· Invalid tier after SVMX1.23 installation.
· Handling of too long zip code.
· Black screen during charging.
· LED strip not working.
· Price and help pop ups are on white background in dark mode.
· The buttons are labelled as Chequing and Savings instead of Chèque and Épargne.
· Installation wizard - site linking fails on 'Fetching site data...'.
· Installation wizard - template values are not applied before SPM pairing screen.
· Installation wizard - the device gets stuck on "Parameters to be saved" screen.
· Installation wizard - add comment to Site linking screen.
· Installation wizard - Hide DHCP button in wizard.
· Installation wizard - install prerequisites should be editable.
· iGem2.5 - Anthem should not retrieve long CAN message unbiasedly.
· update welcome screen text.
· Anthem does not return to correct screen after nozzle lifted too early. 
· Face detection throws error.
· Anthem does not disable UI when other fueling point has taken control of pre-fueling.
· Anthem does not react to stopping sequence.
· Hydrogen - When Button NO is pressed on Confirm Screen Anthem should send Lock Grades Message.
· Language selection removed from Locked Idle Screen
· Anthem forgets Pre-Fulling control if filling is ongoing.
· Grade buttons unlocked before user confirmed that they can operate the equipment.
· Remove the Default Verifone config from the system.
· Malfunctioning of grades config cloning.
· Installation wizard - Internet connection verification malfunctioning.
· The SPM status does not change after Force Unpair.
· Statuses of SPM devices on Maintenance Screen need rephrasing.
· Anthem does not react correctly to nozzle lift before grade select.
· Update UI for charging screens - price vs. power delivered.
· RED BARN MARKET 11 - HW issue, Pop-up modal displayed on screen, "“The instruction at 0x00007FFBEBF4EA91 referenced memory at 0xFFFFFFFFFFFFFFFF. The memory could not be read.
· Anthem Logs between 1.20.5 and 1.22.0 are significantly different.
· EV needs to install both at once, default and EV help.

1.22.0 – 04/18/2024

· Copy tiering files between dispensers
· Remove branding restrictions from tiering
· Custom Configurations for individual Vendors
· To check SPM2 availability before logs downloading via DX-Monitor/iSense
· Move time zone selection to Set date/time window
· Add RFID status to diagnostics screen
· Add internet speed test
· Pass through rework
· SPM reboot to be optional
· Disable saving configuration without EN language selected
· Add Gilbarco default prompt mapping file to configuration
· Update folder structure for SPM2 related configuration
· Update Anthem Help files with Installation Manual
· Add basic troubleshooting information
· Update system prompts to alternative language once changed by POS
· Anthem 27'' ADA button available for 3rd party only
· Preview of 3rd party apps
· Display health monitoring screen once Anthem is turned on in factory mode
· Update button label for loading configuration
· Block software copying when source dispenser has older SW version
· Show scanner status in the Health Monitoring screen
· Copy software between dispensers from UI
· 3rd party apps preview
· Add 'more' button on Anthem
· SPM's nightly reboot is triggered from Anthem during transaction
· Upgrade to .NET8
· Regression testing 1.22
· Refactor prompt sequencer
· System Information refactoring
· Performance testing of new boards
· Enable sending template files from CM to Anthem
· Design installation wizard steps
· Unit Price update for iGem 2.5
· Anthem - Standardization work - pump controller
· Rework the way data is copied between dispensers
· Cleaning mode rework
· Anthem incorrect pop reported with .xml file/ datetime format incorrect for idle and fueling.
· A27 dispenser- In POP report static ads being played is recorded at duration every day without fueling
· POP Report is not getting all the media FUELING/IDLE videos
· Icons missing
· Screen does not refresh when enable softkey command is sent after DisplaySecurePrompts
· When scanner is not in the system should be greyed out in health monitoring
· File replication got interrupted by a SPM reset
· EMV 3.1 (Anthem): EnableFunctionKeysCommand is not displaying soft keys on Anthem with secure prompts
· Contactless Tap Does not Cancel Burn-In Protection
· Scanner Status Misreported on Maintenance
· SPM connection issues after Force Unpair
· Links in the Anthem Help panel
· SPM is paired but 'not connected' after reboot of Anthem board
· Configuration/branding coping malfunction
· Default contrast property changes after update from SVMX 1.15 to 1.22
· WPF occurs during transaction - Passthru (Verifone)
· Change button name from "Hosted Apps Test" to "Hosted Apps Preview"
· EMV to be capitalized in Diagnostics screen
· [EVC] RFID reader cannot be detected due to random COM port assignment in OS
· [EVC] Connecting the car does not disable screen burn protection
· [EVC] Connecting and disconnecting the outlet causes an 'session error'
· The 'Configuration' button disappears after entering Dispenser Health Monitoring
· Need to map Idle and Fueling prompts for GVR
· Language changes and flickers with no control during transaction
· The Secure Prompts for the Gilbarco Config for Anthem are wrong
· AnthemNavKeyMode default needs to be set to false, cause POS systems not to boot.
· WPF.1007 occurs after using debit card. Variant - Pass Thru
· Need to add the updated Gilbarco Configurations to be publish for Potential Beta test
· "pay here debit" button on the main Anthem screen
· 1.21 - Presentation mode interferes with Diagnostic Card Reader test and exits runtime diagnostics maintenance menu
· WPF.0 and WPF.1019 displayed due to Prompt.Verifone.PassThru.json missing Prompt ID "1019" to screen name "transaction-cancelled", and Prompt ID "0" to screen name "wait-display-prompt".
· Fix IxPaySimulator
· Incorrect display of Table in UI
· Printer information is invalid
· DHCP - pairing request does not contain IP address
· System Information Only Shows 1 of 3 URLs
· Cloud connection URLs have changed order
· Copy software between dispensers on site
· Removed branding restrictions from tiering
· Custom EMV configurations in configuration default package
· Time zone selection dropdown added to Date/Time screen
· Preview of 3rd party apps added as diagnostic option
· Scanner status displayed in Health monitoring screen
· Configurable setting to reboot SPM after software installation is completed


1.20.5 – 01/17/2024

· Move time zone selection to Set date/time window
· SPM reboot to be optional
· POP Report is not getting all of the media FUELING/IDLE videos
· File replication got interrupted by a SPM reset
· EMV 3.1 (Anthem): EnableFunctionKeysCommand is not displaying soft keys on Anthem with secure prompts.

1.20.4 – 08/09/2023

· System information Only Shows 1 of 3 URLs
· Cloud connection URLs have changed order

1.20.3 – 08/02/2023

· Remove Anthem registration using IEP service

1.20.2 – 07/28/2023

· When no connection to IEP, connect to cloud serviceeusing the old way
· Reboot SPM, once Anthem is in COIPA
· Reset DeviceSiteCodeUrl on production if it points to QA env

1.20.1 – 04/21/2023

· ANTHM-6685: Added “Enter Driver’s License prompt
· ANTHM-6723: Touch detect application in wet environment
· ANTHM-6962: Enable change of date/time format
· ANTHM-6884: Added tier related functions to SVMX
· ANTHM-6885: SAM functions based on tiers
· ANTHM-7012: Configuration update delta in SVMX
· ANTHM-6890: Allow pay inside when no SPM
· ANTHM-6963: Play media sound once fueling is started
· ANTHM-6852: Display media content in Presentation mode
· ANTHM-7063: Display media in Billboard mode
· ANTHM-7072: Enhanced carwash
· ANTHM-7146: Added occasional themes for Anthem backgrounds
· ANTHM-7197: Device registration to IOT hub
· ANTHM-7202: Updated SVMX folder structure for theme images
· ANTHM-7104: Proof of play support for external URL’s
· ANTHM-7268: ADA related updates for 3rd party apps 27” screen
· ANTHM-7303: Configurable time for DR being displayed on screen
· ANTHM-7199: scanner beeps once barcode is scanned
· ANTHM-7267: Send SPM firmware updated only after SW version is different
· ANTHM-7195: Installation of 12/27” touch driver depending on screen size
· ANTHM-7196: Initialize system reference for 12” screens during touch driver installation
· ANTHM-7424: Updated tiering information displayed and sent to DX Monitor
· ANTHM-7510: Add replication status information to Health check and Pairing screen 
· ANTHM-7496: Update default application settings for SVMX 1.20 
· ANTHM-7491: CM - There should not be any disabled features in Instance configuration screen for Tier 4 
· ANTHM-7517: Prompt mapping issue with 1.9.2.756 Prompt.Verifone.json file 
· ANTHM-7490: Dispenser stuck on PIN entry screen during EMV transaction (SPM and SVMX connection issues) 
· ANTHM-7469: 1.7.0 Branding Config file from a previously installed Branding pack is transferred with 1.13.0 Branding pack during Load Configuration. 
· ANTHM-7446: SpecialSoftKeysMap for Help and Cancel soft keys did not display correctly on pressing the Pay Inside key, they should not display vertically 
· ANTHM-7432: CM: Dispenser Tier Not Considered
· ANTHM-7274: Paper receipt is not printed (Gilbarco/Passport POS)
· ANTHM-7235: Poor responsiveness of carwash buttons
· ANTHM-7269: Invalid data in runtime information file

1.19.2 - 12/8/2022

· ANTHM-7072: Add carwash buttons' configuration to Anthem settings
· ANTHM-7146: Add occasional theme as Anthem background

1.19.1 - 12/06/2022

· ANTHM-7063: Display media in "billboard mode"

1.19 - 08/24/2022

· ANTHM-6114: Clone config/brand from nearest pump on the same station - design
· ANTHM-6370: A12 touch driver configuration
· ANTHM-6286: Prepare "camera panel" presenting camera preview screen and allowing to scan QR code
· ANTHM-6182: Car wash image configurable via DX Promote - implementation
· ANTHM-5737: Targeted media content based on consumer grade selection
· ANTHM-6326: Fuel Additive configurable via DX Promote - implementation
· ANTHM-6567: Improve messaging in SAM during installation process
· ANTHM-6719: Disable cache for system HDD via Update Assistant
· ANTHM-6499: Use UserPortal code to allow send digital receipts (allow SPM to send receipt to SVMX)
· ANTHM-6770: Allow car wash image to be displayed as "full panel background"
· ANTHM-6777: Screen mode scheduling configuration
· ANTHM-6771: Allow 5 fuel grades to be displayed without carousel
· ANTHM-5771: Screen burn in protection
· ANTHM-6963: Turn on media sound once start fueling SVM12" standalone
· ANTHM-6890: Allow indoor payment - update logic and prompt mapping
· ANTHM-6330: SVMX Applications - migration from .net core 2.2 to .net 6
· ANTHM-6427: [SVMX] Move presence detection to frontend

1.18.5 - 12/09/2022

· Car wash functionality and panels
1.18.4 - 10/05/22

· ANTHM-6964: SVMX 1.18.3.884 - Carwash screen persists after car wash select prompt

1.18.2 - 08/03/2022

· ANTHM-6457: Decimal point handling during entry
· ANTHM-6450: No grades animation on carousel when changing the language
· ANTHM-6441: GSDG Client does not restart after DFS Wireless Subscriber Units lose forecourt communication
· ANTHM-6451: Carousel speed incorrect when changing language

1.18.1 - 06/24/2022

· ANTHM-6613: iSenseController failed to send Device Registration properties to DX Monitor
· ANTHM-6492: Anthem: Failed to display Secure prompt AdditionalPromptText, instead displays "ClearTextEntry.ClearText1007"
· ANTHM-6496: Anthem: EMV Kernel % variables are not recognized by Anthem for displaying secure prompts
· ANTHM-6469: Anthem display CustomerAppUI issue failed to render the AdditionalText "Fueling", instead it shows [object Object]
· ANTHM-6620: Intercom activation fails randomly when activated via physical button
· ANTHM-6616: Languages as default unchecked after 1.18.1 fresh install 
· ANTHM-6424: Anthem, Create an Image for a USB stick that can Unlock Anthem SW for RMA test.
· ANTHM-6534: Enabled languages selector

1.18 - 01/26/2022

· ANTHM-5950: Missing the DUKPT key injection Index function for EMV in Anthem UI
· ANTHM-5777: Fuel Theft warning message
· ANTHM-4783: GSDG API address should be set automatically by the application
· ANTHM-5792: ADA - Use navigation keys on SPM for screen prompts
· ANTHM-6033: Disable auto select grade for one-product nozzle
· ANTHM-6102: Add the firmware version and BIOS version to system information screen
· ANTHM-6423: Factory restore problem on "NEW OS" 
· ANTHM-6292: Prompt mapping configuration improvements
· ANTHM-6534: Enabled languages selector
· ANTHM-4032: RabbitMQ - Convert all modules to support queueing of messages
· ANTHM-6090: Change the way configuration changes are propagated
· ANTHM-6097: IxPaySimulator improvements
· ANTHM-6136: Refactor UltimateSimulator
· ANTHM-6113: Unclear behavior and wrong messages on the screen during Force Unpair
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